C:\Users\sfdg\Desktop 
architecture =  

  A: D8CB8A00759A
 ============================= AFUWIN 3.06.01 ================================
 ================================ AFU3 END ===================================

Intel (R) Flash Programming Tool. Version:  8.1.51.1476 
Copyright (c) 2007 - 2013, Intel Corporation. All rights reserved.


Error 201: [FPTw.exe] cannot be run on the current platform.
Please contact your vendor.

Intel (R) Flash Programming Tool. Version:  9.1.2.1000 
Copyright (c) 2007 - 2014, Intel Corporation. All rights reserved.

Platform: Intel(R) Q87 Express Chipset 
Reading HSFSTS register... Flash Descriptor: Valid 

    --- Flash Devices Found ---
    MX25L6405D    ID:0xC22017    Size: 8192KB (65536Kb)
    MX25L3205D    ID:0xC22016    Size: 4096KB (32768Kb)

    --- Flash Image Information --
    Signature: VALID
    Number of Flash Components: 2
        Component 1 - 8192KB (65536Kb)
        Component 2 - 4096KB (32768Kb)
    Regions:
        Descriptor - Base: 0x000000, Limit: 0x000FFF
        BIOS       - Base: 0x580000, Limit: 0xBFFFFF
        ME         - Base: 0x003000, Limit: 0x57FFFF
        GbE        - Base: 0x001000, Limit: 0x002FFF
        PDR        - Not present
    Master Region Access:
        CPU/BIOS - ID: 0x0000, Read: 0x0B, Write: 0x0A
        ME       - ID: 0x0000, Read: 0x0D, Write: 0x0C
        GbE      - ID: 0x0118, Read: 0x08, Write: 0x08
 Based on the Host Region FRACC the Host/CPU/BIOS has ( 0x00004A4B ) : 
             Read    Write  
    Desc  :  Yes      No 
    Host  :  Yes     Yes 
    ME    :   No      No 
    GbE   :  Yes     Yes 
    PDR   :   No      No 

Total Accessable SPI Memory: 12288KB, Total Installed SPI Memory : 12288KB

FPT Operation Passed

Intel (R) Flash Programming Tool. Version:  9.5.14.1724 
Copyright (c) 2007 - 2013, Intel Corporation. All rights reserved.

Platform: Intel(R) Q87 Express Chipset 
Reading HSFSTS register... Flash Descriptor: Valid 

    --- Flash Devices Found ---
    MX25L6405D    ID:0xC22017    Size: 8192KB (65536Kb)
    MX25L3205D    ID:0xC22016    Size: 4096KB (32768Kb)

    --- Flash Image Information --
    Signature: VALID
    Number of Flash Components: 2
        Component 1 - 8192KB (65536Kb)
        Component 2 - 4096KB (32768Kb)
    Regions:
        Descriptor - Base: 0x000000, Limit: 0x000FFF
        BIOS       - Base: 0x580000, Limit: 0xBFFFFF
        ME         - Base: 0x003000, Limit: 0x57FFFF
        GbE        - Base: 0x001000, Limit: 0x002FFF
        PDR        - Not present
    Master Region Access:
        CPU/BIOS - ID: 0x0000, Read: 0x0B, Write: 0x0A
        ME       - ID: 0x0000, Read: 0x0D, Write: 0x0C
        GbE      - ID: 0x0118, Read: 0x08, Write: 0x08
 Based on the Host Region FRACC the Host/CPU/BIOS has ( 0x00004A4B ) : 
             Read    Write  
    Desc  :  Yes      No 
    Host  :  Yes     Yes 
    ME    :   No      No 
    GbE   :  Yes     Yes 
    PDR   :   No      No 

Total Accessable SPI Memory: 12288KB, Total Installed SPI Memory : 12288KB

FPT Operation Passed

Intel (R) Flash Programming Tool. Version:  9.6.0.1038 
Copyright (c) 2007 - 2013, Intel Corporation. All rights reserved.

Platform: Intel(R) Q87 Express Chipset 
Reading HSFSTS register... Flash Descriptor: Valid 

    --- Flash Devices Found ---
    MX25L6405D    ID:0xC22017    Size: 8192KB (65536Kb)
    MX25L3205D    ID:0xC22016    Size: 4096KB (32768Kb)

    --- Flash Image Information --
    Signature: VALID
    Number of Flash Components: 2
        Component 1 - 8192KB (65536Kb)
        Component 2 - 4096KB (32768Kb)
    Regions:
        Descriptor - Base: 0x000000, Limit: 0x000FFF
        BIOS       - Base: 0x580000, Limit: 0xBFFFFF
        ME         - Base: 0x003000, Limit: 0x57FFFF
        GbE        - Base: 0x001000, Limit: 0x002FFF
        PDR        - Not present
    Master Region Access:
        CPU/BIOS - ID: 0x0000, Read: 0x0B, Write: 0x0A
        ME       - ID: 0x0000, Read: 0x0D, Write: 0x0C
        GbE      - ID: 0x0118, Read: 0x08, Write: 0x08
 Based on the Host Region FRACC the Host/CPU/BIOS has ( 0x00004A4B ) : 
             Read    Write  
    Desc  :  Yes      No 
    Host  :  Yes     Yes 
    ME    :   No      No 
    GbE   :  Yes     Yes 
    PDR   :   No      No 

Total Accessable SPI Memory: 12288KB, Total Installed SPI Memory : 12288KB

FPT Operation Passed

Intel (R) Flash Programming Tool. Version:  1.0.4.1089 
Copyright (c) 2007 - 2013, Intel Corporation. All rights reserved.


Error 201: [FPTw.exe] cannot be run on the current platform.
Please contact your vendor.

Intel (R) Flash Programming Tool. Version:  1.1.1.1120 
Copyright (c) 2007 - 2014, Intel Corporation. All rights reserved.


Error 201: [FPTw.exe] cannot be run on the current platform.
Please contact your vendor.

Intel (R) Flash Programming Tool. Version:  10.0.30.1054 
Copyright (c) 2007 - 2014, Intel Corporation. All rights reserved.

Platform: Intel(R) Q87 Express Chipset 
Reading HSFSTS register... Flash Descriptor: Valid 

    --- Flash Devices Found ---
    MX25L6405D    ID:0xC22017    Size: 8192KB (65536Kb)
    MX25L3205A    ID:0xC22016    Size: 4096KB (32768Kb)

    --- Flash Image Information --
    Signature: VALID
    Number of Flash Components: 2
        Component 1 - 8192KB (65536Kb)
        Component 2 - 4096KB (32768Kb)
    Regions:
        Descriptor - Base: 0x000000, Limit: 0x000FFF
        BIOS       - Base: 0x580000, Limit: 0xBFFFFF
        ME         - Base: 0x003000, Limit: 0x57FFFF
        GbE        - Base: 0x001000, Limit: 0x002FFF
        PDR        - Not present
    Master Region Access:
        CPU/BIOS - ID: 0x0000, Read: 0x0B, Write: 0x0A
        ME       - ID: 0x0000, Read: 0x0D, Write: 0x0C
        GbE      - ID: 0x0118, Read: 0x08, Write: 0x08
 Based on the Host Region FRACC the Host/CPU/BIOS has ( 0x00004A4B ) : 
             Read    Write  
    Desc  :  Yes      No 
    Host  :  Yes     Yes 
    ME    :   No      No 
    GbE   :  Yes     Yes 
    PDR   :   No      No 

Total Accessable SPI Memory: 12288KB, Total Installed SPI Memory : 12288KB

FPT Operation Passed
